University of Toronto, Department of Electrical and Computer Engineering

ECE241F -Corrected Header/MAX 7128 Pin Correspondence

* indicates the pins for which the original handout were incorrect

Protoboard Header #

MAX 7128 Pin (or board signal)

Protoboard Header #

MAX 7128 Pin (or board signal) 1 Raw (beware! don’t use) 2 Ground 3 Vcc 4 Ground 5 Vcc 6 Ground 7 No Connect 8 No Connect 9 No Connect 10 No Connect 11 No Connect 12 GCLRn/1 13 OE1/84 14 OE2/GCLK2/2 15 4 16 5 17 6 18 8 19 9 20 10 21 11 22 12 23 15 24 16 25 17 26 18 27 20 28 21 29 22 30 25 * 31 24 * 32 27 33 29 * 34 28 * 35 31 * 36 30 * 37 33 38 34 39 35 40 36 41 37 42 40 * 43 39 * 44 41 45 44 46 46 * 47 45 * 48 48 49 50 * 50 49 * 51 52 * 52 51 * 53 54 54 55 55 56 56 57 57 Vcc 58 Ground 59 Vcc 60 Ground